|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 品牌 | 型号 | 图片 | 简介 | 价格 | 备注 |
| Thermo Fisher （美国） | RadEye PRD 19-155-224 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\TXA`HN$8NG~Q1R@D}[F}Q{7.jpg | RadEye PRD Safety Kit, detector calibrated in R/h, with 59in. extension | $2,330.00 | https://www.fishersci.com/shop/products/thermo-scientific-radeye-prd-personal-radiation-detector-4/p-3274592 |
| RadEye PRD 19-155-225 | RadEye PRD Safety Kit,detector calibrated in R/h, with 157in. extension | $2,500.00 |
| RadEye PRD 19-155-226 | RadEye PRD Safety Kit, detector calibrated in Sv/h, with 59in. extension | $2,275.32 |
| RadEye PRD 19-155-227 | RadEye PRD Safety Kit, detector calibrated in Sv/h, with 157in. extension | $2,500.00 |
| Mirion （芬兰） | DMC 3000 Electronic radiation dosimeter | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\}5)ZLWRD0Q9Z8M(SC8H53{L.jpg | It features superior gamma and X-ray energy response, programmable alarms with visual LED, audible, and vibrating alarm indicators, simple 2-button navigation, and the ability to be fitted with external modules for expanded capabilities | Call for prix | https://www.mirion.com/products/dmc-3000-electronic-radiation-dosimeter/ |
| DMC 3000 Module | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\EX_2XUS83`ETKIYYW}X_3OU.jpg | The add-on Beta Module attaches to the DMC 3000 dosimeter and provides Hp(0,07) with a wide range of beta radiation measurement |  |
| DMC 3000 NEUTRON MODULE | The add-on Neutron Module attaches to the DMC 3000 dosimeter and provides a wide range of Hp(10) Neutron radiation measurement. |  |
| DMC 3000 TELEMETRY MODULE | The add-on Telemetry Module attaches to the DMC 3000 dosimeterand allows transmission of a worker’s radiological data to the WRM2 base station and software for remote monitoring. The Telemetry module also allows for additional connected accessories like the heart rate monitor and alarm enhancments. Supplemental power allows for 40+ hours of continuous use. |  |
| RDS-31s | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\B2DD8P3_F3Q3S61AYUI3_UC.jpg | The RDS-31 is a compact GM tubed-based handheld gamma radiation detector.  The RDS-31 is complemented by a full line of external probes to detect alpha and beta radiation. |  | <http://www.hesppe.com/hesppe-344.html> （中文介绍） |
| RDS-30  Radiation Survey Meter | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\F1RTOU2M[12JMESM@%4OIQB.jpg | The RDS-30 is a Digital Handheld Dose Rate Meter designed for a wide range of applications.  Perfect for first responders, civil defense, industrial radiography, or as a radiation survey tool for oil & gas pipelines. |  |
| Step-sensor (德国) | Survey Meter OD-01 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\6Z@5]0VCW6O~WW~9IC]WJAX.jpg | 3 decades for dose and 6 decades for dose rate measurements：hard Xray， soft-radiation region and gamma，beta |  | http://step-sensor.de/en/strahlenmesstechnik/ortsdosimeter.html |
| Survey Meter PM1405 (Polimaster) | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\MJNDJORZK}_@J1)2%TPGAM4.jpg | Measurement of  the ambient dose rate equivalent of gamma radiation, X-ray and beta radiation flux density |  |
| Survey Meter SM 3D | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\02IU219_RWPF8RB_TH`VICD.jpg | Portable, digital pocket radiometer for measurement of the ambient dose rate equivalent dH\*(10)/dt. (Dose rate display range: 0 ... 999 µSv/h) |  |
| Survey Meter SM 5D | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\RZC4QU6I8_)[Z7KU`QP@XF9.jpg | Portable, digital pocket radiometer for measurment of the dose rate equivalent of X-rays and gamma radiation and for the measurement of the area activity of alpha and beta radiation (Area activity: 0 .. 199 Bq/cm², Dose rate: 0 .. 300 µSv/h) |  |
| Survey Meter SM 5D | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\Q@9]M5GRDBL}79~_C}QCOG4.jpg | Detecting of food contaminations; Measuring the pulse rate of 0.1 to 2000 cps |  |
| Electronical multi-use dose meter PM1203M (Polimaster) | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\TI@N)ARWV)7~I}AY~209~59.jpg | Measurement of the ambient dose equivalent H\*(10) and ambient dose rate equivalent dH\*(10)/dt |  |
| InternationalMedcom （美国） | Radalert 100X Radiation Detection Meter | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\}T`Z~32N~V~PN(0FZR9IF$0.jpg | The Radalert 100X is a general purpose geiger counter that measures alpha, beta, gamma, and X-radiation. Features of the Radalert 100X, include a three-second update and a Utility Menu | $450.00 | http://www.amazon.com/International-Medcom/b/ref=bl\_dp\_s\_web\_3517256011?ie=UTF8&node=3517256011&field-lbr\_brands\_browse-bin=International+Medcom |
|  | CRM-100 Digital Radiation Monitor | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\J8CF9492}N]12UF3G$HZT(6.jpg | a hand-held radiation detector that detects potentially harmful ionizing alpha and beta particles, and gamma and x-ray radiation, and features an accumulated total timer function, a Geiger-Mueller (G-M) tube, and LCD digital display of milliroentgens (mR) per hour (mR/hr), counts per minute (CPM), microSieverts (μSv) per hour (μSv/hr), or counts per second (CPS). | $350.00 |  |
| Quarta Rad  (Russie) | RADEX One | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\5K{5R$V`74WB78N45X@ABAW.jpg | RADEX ONE provides a non-professional consumer with fast and precise measurements that can be used for localisation of high-level radioactive sources.  Detect β (Beta), γ (Gamma) and X-ray radiation | $98.95 | http://quartarad.com/product-category/radiation-detector/ |
| RADEX RD1008 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\KPIR4{SXW[{Q`KC(TKCCRAU.jpg | The first handheld radiation detector that detects and displays radiation results for Beta- and Gamma- as two separate values. simultaneous and separate evaluation of Gamma- and Beta-particles; | $349.95 |
| RADEX RD1212  RADEX-RD1212-BT | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\GA7[4}ISDU$_4DV_SGL`R37.jpg | Comes with a USB-to-PC cable and RadexRead Software. RadexRead allows you:  Detect and Measure β (Beta), γ (Gamma) and X-ray Radiation | $209.95  $239.95 |
| RADEX RD1503+ | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\(D3_ASC)~J`H$KGI[_P5`~4.jpg | Detect and Measure β (Beta), γ (Gamma) and X-ray Radiation  Graduated threshold of Audio alarm with 9 levels in range from 0.10 to 0.90 µSv/h | $148.95 |
| RADEX RD1706 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\WBNN`9J}}X{JX`815)OCI9F.jpg | 最新進口的RD1706型X、γ和β輻射檢測儀，是同類産品中性價比最高的輻射檢測儀，此輻射檢測儀廣泛用在放藥生産科研單位，各種實驗室，核電廠，採石場，緊急狀況營救站，金屬處理廠，地下油田和供油管道裝備，室內建築物，建築原材料，環境保護等部門等場所，適用於工作在電離輻射環境中的工作人員。  RD1706在RD1503 和RD1503 +的基礎上經多次改進而成，大大縮短輻射測量時的觀測時間，顯示範圍也有提高，擁有了更精確的檢測X線的輻射的能力， RADEX RD1706非常方便地運用於室內建築物及建築材料的檢測，RADEX RD1706保留了RD1503 +的所有後臺操作模式，作爲報警系統的另外一個特點的震動信號也保留了下來。  RADEX RD1706擁有一個SBM20-1型 的G-M硬β放射線和一個γ放射線探測器，其典型的技術包括：縮短了輻射測量時間，提高了顯示範圍，並且提高了測量精確度，指示範圍從0.05µSv/h-999,0 µSv/h，檢測時間從原來的26秒降到1秒，這對工作在電離輻射環境下的工作人員提供了可靠的保護。 | $249.95 |
| Coliy （德国） | R500 多功能数字辐射仪 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\{)MB~FPQ1O$UAC5I[KS(OIP.jpg | 特制防污套，避免人员和仪器受到污染，双重保护传感器 伸缩杆可远距离测量核射线，避免人体受到伤害（选配） 无线传输2KM距离,或有线RS485传输1.2KM距离 |  | http://www.coliy.cn/cn/chanpin/hefushejianceyiqi/ |
| R700 多探头核辐射仪 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\IQMD_1XI$RCY[)1C{68}6MV.jpg | 3.2英寸全屏彩色触摸屏  主机自动识别探头  新增本底移除功能，可移除95%的本底 大屏幕可同时显示时间，实时值，最大值、最小值，报警阈值 |  |
| R800 多任务核辐射仪 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\6]V7%@OPKAHW5GH3I8)WF9N.jpg | 高灵敏度大面积半导体传感器 传感器表面有超薄铝涂层保护，不易破损  可分辨出α、β、γ射线类别及其强度 可选α能谱分析功能 彩色TFT阳光可视显示屏 可显示多种测量结果，还可显示趋势图 既可以作为巡检仪，还可作为表面污染仪检测使用 |  |
| R910 多功能数字核辐射仪 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\J1JC_AO_8ZKO~_2`OMCU(%P.jpg | 本底跟踪算法，实现高稳定度及快速响应 射线选择开关：对α、β、γ和X射线进行组合选择  可进行辐射剂量值累计 |  |
| Polimaster （白俄罗斯） | PM1401K / KM | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\OPM774AV%ANJMJ7ASLL4}HK.jpg | The small-size light-weight multipurpose radiation monitor for detection of alpha, beta, gamma and neutron radiation sources. Recommended for wide range of radiation monitoring procedures. |  | http://www.polimaster.com/products/compare/?item%5B%5D=224&item%5B%5D=86&compare.x=93&compare.y=1 |
| Multipurpose Hand-Held Radiation Monitor/Identifier - РМ1401К-3/M | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\UK(XHH{T$_EYB`RCTVGFH2R.jpg | the latest modification of РМ1401К/М series, which proved to be successful among radionuclide identifiers with a large number of users.  РМ1401К-3 combines the functionality of personal *radiation detector, survey meter, activity monitor* and *radioisotope identifier*. |  |
| PM1403 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\N9NZ`W%{C6WO}6Q5[0NZ__S.jpg | The device is equipped with a built-in CsI(TI) detector for detection and location of gamma radiation sources and reliable identification of radioisotopes. In addition, the device has five external interchangeable modules for detection of alpha, beta, gamma and neutron radiation. |  |
| 恒奥德 | HA-RM2050 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\IEJA_JSM]@NR~4OIZE01@%4.jpg | HA-RM2050  αβγX射线辐射检测仪是用于测量α、β辐射表面污染和γ、X射线剂量率的智能化检测仪器，采用进口探测器,能同时测量α、β、γ、X射线。该仪器采用低功耗单片机设计,图文式液晶显示,操作简便,广泛应用于环境监测、卫生防疫、无损检测、核医学、进出口商检、放射医疗、建材、纺织、石油化工、分子生物学、核实验室等领域的放射性工作场所的工作台面、地板、墙壁及工作人员的手、脚、衣服等表面的α、β放射性污染检测以及γ剂量率监测。 |  |  |
|  | HA-R280 | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\_2XDIZZ76)~3K]65BI4R[KC.jpg | 多功能数字辐射检测仪/射线检测仪/β、γ和Χ射线分析仪 |  |  |
| GQ | GMC-300E-Plus | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\9SE5%ODAIG%`EZ6FBFH[X[5.jpg | GQ GMC-300E-Plus Digital Geiger Counter Nuclear Radiation Detector Monitor Meter dosimeter Beta Gamma X ray data logger recorder realtime monitoring test equipment | $99.00 |  |
|  | GMC-320-Plus | C:\Users\qian\AppData\Roaming\Tencent\Users\563174213\QQ\WinTemp\RichOle\A}TRYV@HRJM4[TVX]U@@CDY.jpg | GQ GMC-320-Plus Geiger Counter Nulcear Radiation Detector Meter Beta Gamma X ray test equipment | $118.00 | http://www.amazon.com/GQ-GMC-320-Plus-Radiation-Detector-equipment/dp/B00I8GQ1EC/ref=lp\_7772837011\_1\_2?srs=7772837011&ie=UTF8&qid=1460593007&sr=8-2 |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |